사  양  서

품명: 고점도접합페이스트혼합장비

○ 주요사양 및 특징

1. 주기기(Main System)

- Mixing type : twist blade rotation & revolution

- Vessel and blade material : SUS304 or higher

- Jacket type vessel for cooling & heating about 10℃ ~ 50℃

- Vessel capacity : 1.4 L

- Vessel working volume : max 1.0 L

- Revolution : 5 ~ 150 rpm

- Blade turning on axis : 10 ~ 300 rpm

- Mixing blade : twist Blade

- Scraper : tafflon

- Mixing motor : server motor

- Lifting method : LM guide

- Hood : vacuum proof type

- Seal method : vacuum proof seal type

- Control : speed, time and temperature

- Sequential control : 2 stage

- Control panel : digital setting & indicator

- Power : AC 220W, 60Hz single-phase

- Dimension : table-top

2. 보조기기(Accessory)

- Spare vessel : 1 ea

- Temperature control water circulator : about 10℃ ~ 50℃

- Syringe filling ram press : 1 L to 150cc

- Vacuum pumping system for degassing

○ 원리 및 특징

- 일반적인 혼합장비는 앵커타입 블레이드를 이용하여 저속으로 장시간 교반하는 방법을 사용하고 있는데, 에폭시 접착제나 솔더페이스트 등과 같은 고점도의 페이스트의 경우에는 분산 및 균질화가 이루어지지 않아 제조가 곤란한데 비해, 트위스트 블레이드의 공전 및 자전을 통한 혼합방법은 고점도의 액상, 분말, 고형물질을 높은 효율로 빠르게 균질화에 도달할 수 있다는 장점이 있다.

○ 기타

- 설치장소까지 운반 및 설치 포함

- 장비사용 교육 포함

- 사용설명서 및 유지보수매뉴얼

- Warranty 1년